{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":28,"n_cols":8,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
["Odd(red) resistor values for ID-Vout1- and for single resistor IDs (i.e. dual heater instruments) are reserved by the autor!"]
["You can use them freely only on ID-Vout2."]
[]
["ID(hex)","ID","R","Rmax","Rmin","ADCmin","ADCmax","ADCnom"]
[1,1,100,{"$f":"C5*1.01","v":101},{"$f":"C5*0.99","v":99},89,93,87]
[2,2,110,111.1,{"$f":"C6*0.99","v":108.9},97,102,{"$f":"(G5+F6)/2","v":95}]
[3,3,120,121.2,{"$f":"C7*0.99","v":118.8},105,110,103.5]
[4,4,130,131.30000000000001,{"$f":"C8*0.99","v":128.69999999999999},113,118,111.5]
[5,5,150,151.5,{"$f":"C9*0.99","v":148.5},128,135,123]
[6,6,180,181.8,178.2,150,157,142.5]
[7,7,200,202,198,164,172,160.5]
[8,8,220,222.2,217.8,177,186,174.5]
[9,9,240,242.4,237.6,190,199,188]
["A",10,270,272.7,267.3,208,219,203.5]
["B",11,300,303,297,226,238,222.5]
["C",12,330,333.3,326.7,243,255,240.5]
["D",13,390,393.9,386.1,273,289,264]
["E",14,430,434.3,425.7,293,309,291]
["F",15,470,474.7,465.3,310,329,309.5]
[10,16,560,565.6,554.4,347,370,338]
[11,17,680,686.8,673.2,389,417,379.5]
[12,18,820,828.2,811.8,432,463,424.5]
[13,19,1000,1010,990,476,514,469.5]
[14,20,1200,1212,1188,517,561,515.5]
[15,21,1500,1515,1485,565,616,563]
[16,22,2000,2020,1980,624,684,620]
[17,23,3000,3030,2970,695,769,689.5]
[18,24,5600,5656,5544,778,870,773.5]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}